**CN-Simulation**

**Code:first.cc**

#include "ns3/core-module.h"

#include "ns3/network-module.h"

#include "ns3/internet-module.h"

#include "ns3/point-to-point-module.h"

#include "ns3/applications-module.h"

#include "ns3/netanim-module.h"

using namespace ns3;

NS\_LOG\_COMPONENT\_DEFINE ("FirstScriptExample");

int

main (int argc, char \*argv[])

{

CommandLine cmd (\_\_FILE\_\_);

cmd.Parse (argc, argv);

Time::SetResolution (Time::NS);

LogComponentEnable ("UdpEchoClientApplication", LOG\_LEVEL\_INFO);

LogComponentEnable ("UdpEchoServerApplication", LOG\_LEVEL\_INFO);

std::string animFile="first.xml";

NodeContainer nodes;

nodes.Create (2);

PointToPointHelper pointToPoint;

pointToPoint.SetDeviceAttribute ("DataRate", StringValue ("5Mbps"));

pointToPoint.SetChannelAttribute ("Delay", StringValue ("2ms"));

NetDeviceContainer devices;

devices = pointToPoint.Install (nodes);

InternetStackHelper stack;

stack.Install (nodes);

Ipv4AddressHelper address;

address.SetBase ("10.1.1.0", "255.255.255.0");

Ipv4InterfaceContainer interfaces = address.Assign (devices);

UdpEchoServerHelper echoServer (9);

ApplicationContainer serverApps = echoServer.Install (nodes.Get (1));

serverApps.Start (Seconds (1.0));

serverApps.Stop (Seconds (10.0));

UdpEchoClientHelper echoClient (interfaces.GetAddress (1), 9);

echoClient.SetAttribute ("MaxPackets", UintegerValue (10));

echoClient.SetAttribute ("Interval", TimeValue (Seconds (1.0)));

echoClient.SetAttribute ("PacketSize", UintegerValue (1024));

ApplicationContainer clientApps = echoClient.Install (nodes.Get (0));

clientApps.Start (Seconds (2.0));

clientApps.Stop (Seconds (10.0));

AnimationInterface anim(animFile);

anim.SetConstantPosition(nodes.Get(0),1.0,2.0);

anim.SetConstantPosition(nodes.Get(1),45.0,60.0);

AsciiTraceHelper ascii;

pointToPoint.EnableAsciiAll(ascii.CreateFileStream("first.tr"));

Simulator::Run ();

Simulator::Destroy ();

return 0;

}

Output:

